

INDUSTRY RESTRICTION LEVELS
Construction: Early stage land development

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| INDUSTRY SPECIFIC REQUIREMENTS | **ACTIONS ACROSS ALL LEVELS** | **CLOSED** | **HEAVILY RESTRICTED***Current - Melbourne* | **RESTRICTED** | **OPEN WITH A COVIDSAFE PLAN** |
| **ENSURE PHYSICAL DISTANCING** | * **Density quotient applied to shared spaces**
* Mark safe distances in work, transit and break areas
* Stagger start times, breaks and finish times
* Manage entry and exit to workplaces
* Personnel lift/hoist controls
* COVIDSafe site induction mandatory for all staff
 | * **All work sites closed except for critical and essential infrastructure, or where required for an emergency**
 | * **Density restrictions of no more than 10 workers per hectare**
* **​**Corporate staff to work remotely and all site offices to apply density quotient
* Manufacturing of building materials will continue to operate as permitted industry
* **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Physical distancing practices
* Minimise work activities in restricted spaces
 | * **Density restrictions of no more than 20 workers per hectare**
* **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Physical distancing practices
* Minimise work activities in restricted spaces
 | * **No restrictions on number of workers per site**
* **High Risk COVIDSafe Plan** in accordance with the latest version of the Construction Industry Guidelines applying a risk-based approach
* Physical distancing practices
* Minimise work activities in restricted spaces
* Workers encouraged to work from home and onsite / office-based activities to resume with density quotient applied,
 |
| **WEAR A FACE COVERING** | * **All staff to wear face coverings as per current directions**
* Provide training/guidance on how to use PPE
* Symptom screening at commencement of shift
 |  | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Face coverings
* Symptom declaration by all workers and visitors accessing site
* Worker declaration at start of each shift
* Temperature testing on site entry (optional)
* PPE information and training
* Monitoring correct use of PPE
 | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Face coverings
* Symptom declaration by all workers and visitors accessing site
* Worker declaration at start of each shift
* Temperature testing on site entry (optional)
* PPE information and training
* Monitoring correct use of PPE
 | * **High Risk COVIDSafe Plan** in accordance with the latest version of the Construction Industry Guidelines applying a risk-based approach
* Face coverings
* Symptom declaration by all workers and visitors accessing site
* Worker declaration at start of each shift
* Temperature testing on site entry PPE information and training
* Monitoring correct use of PPE
 |
| **PRACTISE GOOD HYGIENE** | * Frequent and regular cleaning and disinfection of shared spaces
* Soap and hand sanitiser available at all workplaces
* Replace high-touch communal items with hygienic alternatives
* Display cleaning log in shared spaces
* Restrict sharing of tools, plants and equipment
 |  | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Cleaning and disinfecting protocols
* Auditing of cleaning schedules
 | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Cleaning and disinfecting protocols
* Auditing of cleaning schedules
 | * **High Risk COVIDSafe Plan** in accordance with the latest version of the Construction Industry Guidelines
* Cleaning and disinfecting protocols
* Auditing of cleaning schedules
 |
| **KEEP RECORDS AND ACT QUICKLY IF STAFF BECOME UNWELL** | * Support staff to stay home and get tested even if they only have mild symptoms
* Have a plan to manage cases, notify others and potentially close down if there are confirmed coronavirus (COVID-19) cases
* Keep records of all people who enter a worksite for contact tracing
 | * Emergency construction responses reported to the Industry Coordination Centre (ICC@ecodev.vic.gov.au) within 6 hours of the event
 | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Workplace mapping and contact tracing procedures in event of confirmed coronavirus (COVID-19) case
* Case notification procedures
* Site closure procedures
* Cleaning and disinfecting regime
* Screening of workers and visitors before accessing the workplace
 | * **High Risk COVIDSafe Plan** in accordance with [Construction Industry Guidelines Version 7](https://www.vba.vic.gov.au/__data/assets/pdf_file/0020/116417/COVID-19-Guidelines-for-the-Building-and-Construction-Industry-Revision-7.pdf)
* Workplace mapping and contact tracing procedures in event of confirmed coronavirus (COVID-19) case
* Case notification procedures
* Site closure procedures
* Cleaning and disinfecting regime
* Screening of workers and visitors before accessing the workplace
 | * **High Risk COVIDSafe Plan** in accordance with the latest version of the Construction Industry Guidelines
* Workplace mapping and contact tracing procedures in event of confirmed coronavirus (COVID-19) case
* Case notification procedures
* Site closure procedures
* Cleaning and disinfecting regime
* Screening of workers and visitors before accessing the workplace
 |
| **AVOID INTERACTIONS IN ENCLOSED SPACES** | * Move as much activity outside as possible
* If possible, do not recirculate air
* No carpooling to work
 |  | * All site induction conducted outside
* All tool box meetings conducted outside
 | * All site induction conducted outside
* All tool box meetings conducted outside
 | * All site induction conducted outside
* All tool box meetings conducted outside
 |
| **CREATE WORKFORCE BUBBLES** | * Minimise movement of workers across sites
* Keep groups of staff rostered on the same shifts for a given geographic area/site
* No overlap in shift changes
 |  |  |  |  |

**Bold – mandatory under public health direction\***Not bold – recommended but not mandated

\*Subject to final development of directions by Chief Health Officer